;     Windows LUFA RNDIS Setup File
; Copyright (c) 2000 Microsoft Corporation

[DefaultInstall]
CopyINF="LUFA RNDIS.inf"

[Version]
Signature="$Windows NT$"
Class=Net
ClassGuid={4d36e972-e325-11ce-bfc1-08002be10318}
Provider=%MFGNAME%
DriverVer=7/1/2012,10.0.0.0

[Manufacturer]
%MFGNAME%=DeviceList, NTx86, NTamd64, NTia64

[ControlFlags]
ExcludeFromSelect=*

[DriverInstall]
Characteristics=0x84 ; NCF_PHYSICAL + NCF_HAS_UI
BusType=15
include=netrndis.inf
needs=Usb_Rndis.ndi
AddReg=Rndis_AddReg_Vista

[DriverInstall.Services]
include=netrndis.inf
needs=Usb_Rndis.ndi.Services

;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------
; When developing your USB device, the VID and PID used in the PC side
; application program and the firmware on the microcontroller must match.
; Modify the below line to use your VID and PID.  Use the format as shown below.
; Note: One INF file can be used for multiple devices with different VID and PIDs.
; For each supported device, append ",USB\VID_xxxx&PID_yyyy" to the end of the line.
;------------------------------------------------------------------------------
[DeviceList]
%DESCRIPTION%=DriverInstall, USB\VID_03EB&PID_204C

[DeviceList.NTx86]
%DESCRIPTION%=DriverInstall, USB\VID_03EB&PID_204C

[DeviceList.NTamd64]
%DESCRIPTION%=DriverInstall, USB\VID_03EB&PID_204C

[DeviceList.NTia64]
%DESCRIPTION%=DriverInstall, USB\VID_03EB&PID_204C

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------
;Modify these strings to customize your device
;------------------------------------------------------------------------------
[Strings]
MFGNAME="http://www.lufa-lib.org"
DESCRIPTION="LUFA RNDIS USB Ethernet Adapter"
