AVRISP-MKII Clone Programmer Project

Macros
LUFAConfig.h File Reference

LUFA Library Configuration Header File. More...

## Macros

#define | ORDERED_EP_CONFIG
#define | USE_STATIC_OPTIONS (USB_DEVICE_OPT_FULLSPEED | USB_OPT_REG_ENABLED | USB_OPT_AUTO_PLL)
#define | USB_DEVICE_ONLY
#define | NO_SOF_EVENTS
#define | USE_FLASH_DESCRIPTORS
#define | NO_INTERNAL_SERIAL
#define | FIXED_CONTROL_ENDPOINT_SIZE 16
#define | DEVICE_STATE_AS_GPIOR 0
#define | FIXED_NUM_CONFIGURATIONS 1
#define | NO_DEVICE_REMOTE_WAKEUP
#define | NO_DEVICE_SELF_POWER

## Detailed Description

LUFA Library Configuration Header File.

This header file is used to configure LUFA's compile time options, as an alternative to the compile time constants supplied through a makefile.

For information on what each token does, refer to the LUFA manual section "Summary of Compile Tokens".

## Macro Definition Documentation

## § DEVICE_STATE_AS_GPIOR

#define DEVICE_STATE_AS_GPIOR 0

## § FIXED_CONTROL_ENDPOINT_SIZE

#define FIXED_CONTROL_ENDPOINT_SIZE 16

## § FIXED_NUM_CONFIGURATIONS

#define FIXED_NUM_CONFIGURATIONS 1

## § NO_DEVICE_REMOTE_WAKEUP

#define NO_DEVICE_REMOTE_WAKEUP

## § NO_DEVICE_SELF_POWER

#define NO_DEVICE_SELF_POWER

## § NO_INTERNAL_SERIAL

#define NO_INTERNAL_SERIAL

## § NO_SOF_EVENTS

#define NO_SOF_EVENTS

## § ORDERED_EP_CONFIG

#define ORDERED_EP_CONFIG

## § USB_DEVICE_ONLY

#define USB_DEVICE_ONLY

## § USE_FLASH_DESCRIPTORS

#define USE_FLASH_DESCRIPTORS

## § USE_STATIC_OPTIONS

#define USE_STATIC_OPTIONS (USB_DEVICE_OPT_FULLSPEED | USB_OPT_REG_ENABLED | USB_OPT_AUTO_PLL)